**HEMI inset round washbasin Ø 385mm**

Bright polished 304 st steel - Recessed inst. from above or below

Reference: **120491**

Specification description

Round washbasin for recessed installation from above or below.

Basin internal diameter: 385mm.

Cut-out diameter: 400mm for installation from above, 380mm for installation from below.

Bacteriostatic 304 stainless steel.

Bright polished finish.

Stainless steel thickness: 0.8mm.

One-piece, seam-free pressed bowl.

Rounded edges prevent injury.

Supplied with 1 ¼" waste.

Without overflow.

CE marked. Complies with European standard EN 14688.

Weight: 1.6kg.

30-year warranty.

[Formerly ref: 0213490301]