**FACIL wall-mounted washbasin**

Polished satin 304 stainless steel

With right tap hole, Ø 35mm

Reference: **121800**

Specification description

Wall-mounted washbasin, 360x390mm.

Basin internal diameter: 310mm.

Clean and simple design.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

With Ø 35mm on the right.

Supplied with 1¼" waste.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 4.1kg.

30-year warranty.

[Formerly ref: 0211080006]