**MINIMAL corner washbasin**

Polished satin 304 stainless steel

With central tap hole, Ø 35mm

Reference: **121550**

Specification description

Wall-mounted corner washbasin (90° angle).

Basin internal diameter: 310mm.

Clean and simple design.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm

Rounded edges prevent injury.

With Ø 35mm central tap hole.

Supplied with 1¼" waste.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 4kg.

30-year warranty.

[Formerly ref: 0211550008]