**Floor-standing ILHA drinking fountain**

Polished satin 304 stainless steel

With built-in tap - H. 915mm

Reference: **180100**

Specification description

Floor-standing drinking fountain.

Bacteriostatic 304 stainless steel. Polished satin finish. Stainless steel thickness: 0.8mm.

Height: 915mm.

Supplied with bubbler tap: chrome-plated, instant shut-offand adjustable flow rate, inlet M⅜".

Flat perforated waste, without screws:easy to clean and vandal-resistant.

Recessed vertical water outlet. Waste outlet 1¼".

Supplied with fixing elements.

Weight: 9.6kg.

30-year warranty.

[Formerly ref: 0810100000]