**Wall-hung 700 S WC pan for disabled people**

Polished satin 304 stainless steel - For people with reduced mobility

Reference: **110710**

Specification description

Wall-hung WC pan, 360 x 350 x 700mm.

Available with 700mm elongated pan for improved comfort for people with reduced mobility (700 S).

Compatible with all standard frame systems available on the market.

Elegant and simple design.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm.

One-piece pressed WC bowl, seam-free for easy maintenance and better hygiene.

WC bowl surface is polished with rounded edges for easy cleaning.

Concealed perimetral flushing rim.

Horizontal water inlet: Ø 55mm.

Horizontal waste outlet: Ø 100mm.

Water saving: works with 4L or more of water.

Shrouded WC pan.

Pre-drilled holes for fixing the toilet seat. Supplied with stainless steel blanking caps when installed without toilet seat lid.

Quick and easy to install from the front thanks to a stainless steel mounting frame.

Supplied with fixing plate and 6 theft prevention TORX security screws.

CE marked. Complies with European standard EN 997 for 4L flush.

Weight: 14.5kg.

30-year warranty.

[Formerly ref: 0112080001]