**L trough urinal**

Polished satin 304 stainless steel - L. 1,200mm - Floor-recessed

Reference: **130210**

Specification description

Floor-recessed trough urinal, 1200 x 1020 x 300mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rear water inlet.

Supplied with 2 stainless steel rinsers and 2 flexible hoses.

Water saving: optimal rinsing with 0.1 L/sec. per service i.e. 0.3L per use.

Central drainage.

Waste outlet 11/2". Supplied with waste and integrated trap (ref. 785000).

Weight: 25.4kg.

[Formerly ref: 0310210001]