**LISO urinal divider for wall-mounting**

Polished satin 304 stainless steel - H. 700mm

Reference: **100590**

Specification description

Urinal divider for wall-mounting.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm.

Smooth surface and rounded edges.

Concealed fixings.

Supplied with fixing elements.

Weight: 8kg.

[Formerly ref: 0011590000]