**DUO S TC R washbasin**

Polished satin 304 stainless steel - Wall-mounted with concealed waste

Without tap hole

Reference: **160360**

Specification description

Wall-mounted washbasin with through-the-wall installation for service ducts.

Integrated countertop.

Basin on the right.

Basin internal diameter: 310mm.

Bacteriostatic 304 stainless steel. Polished satin finish. Stainless steel thickness: 1.2mm

Rounded edges prevent injury.

Vandal-resistant: shrouded basin, concealed waste outlet.

200mm threaded rod can be cut to size (other lengths are available on request).

Recessed horizontal waste outlet Ø 1".

Flat perforated waste, without screws: easy to clean and vandal-resistant.

Without overflow. Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 8.5kg.

[Formerly ref: 0216360000]