**KOMPACT washbasin and wall-hung WC combination**

Polished satin 304 stainless steel - Wall-mounted - Central WC

Reference: **160500**

Specification description

Combination unit: washbasin and WC pan suspended centrallywith recessed toilet roll holder.

Wall-mounted installation with 3 access panels, 2 on the sidesand 1 on the top with theft prevention TORX security screws.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel unit thickness: 2mm.

Rounded corners and edges for improved safety.

Smooth surface for easy cleaning.

Suitable for prisons, police stations, etc.

WC pan is completely welded to washbasin, no screws:

makes cleaning easier and prevents concealment of objects.

Washbasin equipped with time flow tap: stainless steel tamperproofpush-button and anti-blocking system, 7 second time flow, M½".

WC equipped with time flow flush valve, 7 second time flow, M¾".

Water inlet: washbasin M½", WC M¾".

Recessed horizontal water outlet: Ø 100mm

Supplied with washbasin siphon.

Easy installation: only one water outlet for both washbasin and WC,water inlet and outlet already connected.

Weight: 36kg.

[Formerly ref: 0610030005]