**Be-line lift-up shower seat**

Wall-mounted removable, lift-up shower seat

Matte white powder-coated aluminium

Reference: **511920W**

Specification description

Be-line® removable lift-up shower seat.

Shower seat for people with reduced mobility.

Wide, designer model.

Removable: easy to remove with anti-theft locking system. Reduces the number of shower seats in a facility, allowing installation only when required e.g. hotels or hospitals providing short-term accommodation for people with reduced mobility.

Retained in upright position. Slowed down descent.

Suitable for intensive use in public places or the healthcare sector.

Solid, reinforced seat made from high strength polymer which can be installed, without a supporting leg, on any suitable wall.

Non-slip surface.

Good resistance to Betadine®.

Mounting bracket made from matte white powder-coated solid aluminium provides a good visual contrast with a dark coloured wall wall.

5 concealed fixing points.

Supplied with stainless steel screws Ø 8 x 70mm for concrete walls.

Dimensions: 455 x 450 x 90mm.

Folded dimensions: 85 x 470mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

Wall-mounted lift-up shower seat with 30-year warranty. CE marked.