**Toilet roll holder, or for spares**

For toilet rolls

Bright polished 304 stainless steel

Reference: **510083P**

Specification description

Wall-mounted toilet roll holder.

Toilet roll holder, or for spares

Can be installed horizontally for standard use, or vertically as a spare toilet roll holder.

Tube Ø 20mm, 1mm thick.

Bacteriostatic bright polished 304 stainless steel.

Concealed fixings.

30-year warranty.