**Be-line® white shower grab bar with sliding shower head holder**

Matte white powder-coated aluminium

Ø 35mm with flat ergonomic face

Reference: **511946W**

Specification description

Be-line® straight bar Ø 35mm with shower head holder for people with reduced mobility.

Can be used as a vertical grab bar and a shower rail for showers or baths.

Matte-white shower head holder with ergonomic locking ring.

Possible to add a sliding soap dish (order separately).

Aluminium tube thickness 3mm. Solid aluminium fixing points.

Rounded profile Ø 35mm with ergonomic flat front face that prevents rotation for an optimal grip.

Matte white powder-coated aluminium provides a good visual contrast with dark walls.

Uniform surface for easy maintenance and hygiene.

38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings.

Supplied with stainless steel screws Ø 8 x 70mm for concrete walls.

Height: 1,050mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

30-year warranty. CE marked.