**DELTA wall-hung urinal**

Polished satin 304 stainless steel - Visible inlet and outlet

Reference: **134710**

Specification description

Wall-hung individual rimless urinal.

Compatible with all standard frame systems on the market.

Bacteriostatic 304 stainless steel. Polished satin finish.

Stainless steel thickness: 1.2mm.

Top (exposed) water inlet.

Recessed or exposed waste outlet. Concealed trap.

Quick and easy to install from the front thanks to a stainless steel mounting frame.

Supplied with 1½" P trap, fixing elements and theft prevention TORX security screws.

CE marked. Complies with European standard EN 13407 for 2L flush.

Weight: 7.5kg.

30-year warranty.