**Wall-mounted SXS mechanical hand washbasin**

Polished satin 304 stainless steel - Knee-operated - with upstand

With tap and premixer

Reference: **182320**

Specification description

Wall-mounted, knee-operated hand washbasin.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 0.8mm.

Rounded edges prevent injury.

With splashback.

Supplied with swan-neck spout, soft-touch operation time flow tap with 7-second time flow and premixer with non-return valves.

Bare version (i.e. without tap) is available (ref. 181320).

Flat perforated waste, without screws: easy to clean and vandal-resistant.

Water savings: flow rate pre-set at 3 lpm.

Maximum hygiene: no manual contact with tap.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 4.3kg.

30-year warranty.