**SECURITHERM dual control shower panel**

Mechanical thermostatic dual control, comfort 10 lpm

Concealed inlet, fixed sh. head + handset, st. st.

Reference: **792354CF**

Specification description

Dual control thermostatic shower panel:

Large model stainless steel shower panel for wall mounted, exposed installation.

Concealed inlet via flexibles M½".

SECURITHERM thermostatic mixer.

Adjustable temperature control from cold water up to 38°C with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding failsafe: automatic shut-off if cold or hot water supply fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Chrome-plated, tamperproof, fixed, ROUND shower head with scale-resistant nozzle and automatic flow rate regulation at 10 lpm at 3 bar.

Handset with removable flexible via rapid push-fit STOP connector, wall support supplied.

Non-time flow valves to control the ROUND shower head and the handset.

Thermal shocks are possible.

Stopcocks.

Concealed fixings.

Filters and non-return valves.

30-year warranty.