**SECURITHERM thermostatic mixer**

Mixer only for mixer set with retracting hand spray

Hygiene control lever L. 100mm

Reference: **H9642**

Specification description

SECURITHERM thermostatic single control sequential sink mixer set with retracting hand spray.

Anti-scalding failsafe: shuts off immediately if cold or hot water supply fails.

Securitouch thermal insulation prevents burns.

Sequential: opens and closes with cold water.

No risk of cross flow between the hot and cold water.

No non-return valves on the inlets.

Scale-resistant thermostatic sequential cartridge for single control temperature and flow-rate adjustment.

Temperature can be adjusted from cold water to 40°C with maximum temperature limiter set at 40°C.

Body with smooth interior.

No manual contact thanks to Hygiene control lever L. 100mm.

Mixed water brass outlet L. 160mm.

PEX flexibles F3/8" and reinforced fixing via 2 stainless steel rods.

30-year warranty.