**Sequential mechanical basin mixer**

Sequential mechanical mixer with swivelling spout L. 200mm

With offset STOP/CHECK connectors

Reference: **2436**

Specification description

Wall-mounted sequential mechanical basin mixer.

Mechanical sequential mixer: opens and closes with cold water within a range of 90°.

Wall-mounted mixer with flat swivelling under spout L. 200mm with hygienic flow straightener.

Securitouch thermal insulation prevents burns.

Ø 35mm classic ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume (reduces bacterial development).

The water velocity in the tubes reduces bacterial development considerably.

Flow rate regulated at 5 lpm.

Chrome-plated brass body.

Hygiene control lever L. 200mm operates requires no manual contact.

Mixer supplied with 2 offset STOP/CHECK connectors M½" M¾" ideal for hospitals.

Recommended installation height: 110 - 200mm above the basin surface.

Mechanical mixer ideal for healthcare facilities, retirement homes, hospitals and clinics.

Sequential mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.