**FINO wall-hung urinal**

Polished satin 304 stainless steel - Rear inlet

Reference: **135710**

Specification description

Wall-hung individual rimless urinal.

Compatible with all standard frame systems on the market.

Bacteriostatic 304 stainless steel. Polished satin finish.

Stainless steel thickness: 1.2mm.

Rear water inlet (recessed).

Recessed or exposed horizontal waste outlet. Concealed trap.

Quick and easy to install to from the front thanks to a stainless steel mounting frame.

Supplied with a 1½" P trap. Supplied with fixing elements.

CE marked. Complies with European standard EN 13407 for a 2-litre flush.

Weight: 3.5kg.

30-year warranty.