**Auto-rewind hose reel**

With 15m flexible hose and hand spray

Reference: **5676T2**

Specification description

Auto-rewind hose reel with flexible hose L. 15m and guide rollers:

Maximum temperature 70°C.

Flow rate 23 lpm at 3 bar.

Maximum pressure 20 bar, 12 bar with trigger-op hand spray.

Hose reel with ABS drum Ø 425mm.

304 Stainless steel bracket.

Order separately: an angled stopcock with integrated vacuum breaker to prevent the back flow of polluted water into the mains supply.

Hose reel with 30-year warranty.