**SECURITHERM EP pressure-balancing basin mixer**

Wall-mounted mixer with swivel spout L .200mm, sculptured lever

With offset STOP/CHECK connectors

Reference: **2445EP**

Specification description

Wall-mounted SECURITHERM pressure-balancing basin mixer.

Wall-mounted mixer with flat, swivelling under spout, L. 200mm with hygienic flow straightener suitable for fitting a BIOFUL point-of-use filter.

Anti-scalding safety: HW flow is reduced if CW fails (and vice versa).

Stable temperature regardless of pressure and flow rate variations in the system.

Securitouch thermal insulation prevents burns.

Ø 40mm pressure-balancing ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume (reduces bacterial niches).

Flow rate regulated at 5 lpm at 3 bar.

Chrome-plated brass body.

Sculptured control lever.

Mixer supplied with offset STOP/CHECK connectors M1/2" M3/4" ideal for hospitals.

Recommended installation height: 110 - 200mm above the basin surface.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.