**SECURITHERM EP pressure-balancing basin mixer**

Wall-mounted mixer with swivel spout L .200mm, Hygiene lever L. 150mm

With offset STOP/CHECK connectors

Reference: **2445LEP**

Specification description

Wall-mounted SECURITHERM pressure-balancing basin mixer.

Wall-mounted mechanical mixer with flat swivelling under spout L. 200mm with hygienic flow straightener,

Spout suitable for fitting a BIOFIL point-of-use filter.

Anti-scalding safety: HW flow rate is reduced if CW fails (and vice versa).

Stable temperature regardless of flow rate and pressure variations in the system.

Mixer with Securitouch thermal insulation prevents burns.

Ø 40mm pressure-balancing ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume.

Flow rate regulated at 5 lpm.

Chrome-plated brass body.

Hygiene control lever L. 150mm requires no manual contact.

Mixer with 150mm centres supplied with offset STOP/CHECK wall connectors M1/2" M3/4" ideal for hospitals.

Filters and non-return valves.

Recommended installation height: 110 - 200mm above the basin surface.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Mixer suitable for people with reduced mobility.

30-year warranty.