**Mechanical basin mixer**

Wall-mounted mixer with swivel spout L .200mm, Hygiene lever L. 150mm

With standard connectors

Reference: **2445LS**

Specification description

Wall-mounted mechanical basin mixer.

Flat, swivelling under spout L. 200mm with hygienic flow straightener suitable for fitting a BIOFIL terminal filter.

Securitouch thermal insulation prevents burns.

Ø 40mm ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume (reduces bacterial niches).

Flow rate 5 lpm at 3 bar.

Chrome-plated brass body.

Hygiene control lever L. 150mm.

Supplied with standard connectors M1/2" M3/4".

Recommended installation height: 110 - 200mm above the basin surface.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Mixer suitable for people with reduced mobility.

30-year warranty.