**Mechanical basin mixer**

Wall-mounted mixer with swivel spout L .200mm, sculptured lever

With standard offset connectors

Reference: **2445S**

Specification description

Wall-mounted mechanical basin mixer.

Mechanical mixer with flat, swivelling under spout L. 200mm with hygienic flow straightener.

Spout suitable for fitting a BIOFIL point-of-use filter.

Mixer with Securitouch thermal insulation prevents burns.

Ø 40mm standard ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume.

Flow rate regulated at 5 lpm.

Chrome-plated brass body.

Sculptured control lever.

Mixer with 150mm centres supplied with offset standard connectors M1/2" M3/4".

Recommended installation height: 110 - 200mm above the top of the basin.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Mixer suitable for people with reduced mobility.

Wall-mounted mechanical mixer with 30-year warranty.