**T-shaped stainless steel grab bar with sliding vertical bar, bright**

UltraPolish bright polished stainless steel

Ø 32mm

Reference: **5441P**

Specification description

T-shaped grab bar with sliding vertical bar Ø 32mm, for people with reduced mobility.

Use as a grab bar and to support the user in an upright position.

Helps and secures entry and movement in the shower.

Use as a shower rail by adding a shower head holder and/or soap dish.

Upright position can be adjusted during installation: can be moved to the left or the right in order to adapt the space (positioning of shower, depth of shower seat...).

Dimensions: 1,160 x 500mm.

Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraPolish bright polished finish, uniform non-porous surface for easy maintenance and hygiene.

Plate welded to the tube by invisible safety bead weld (process exclusive to "ArN-Securit").

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings secured to wall by a 3-hole fixing plate, Ø 72mm.

Fixing and cover plates in 304 stainless steel.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight: 135kg.

 30-year warranty. CE marked.