**TEK washbasin**

Polished satin 304 stainless steel - Wall-mounted - Concealed drainage

With integrated tap

Reference: **161340**

Specification description

Wall-mounted washbasin.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

Vandal-resistant: shrouded basin, concealed trap.

Supplied with 1 time flow tap: stainless steel tamperproof push-button and anti-blocking system, 7 seconds time flow.

Flat perforated waste, without screws: easy to clean and vandal-resistant.

Without overflow.

Supplied with trap.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 8.6kg.