**TEK washbasin**

Polished satin 304 stainless steel - Wall-mounted - Concealed drainage

With integrated electronic tap

Reference: **161440**

Specification description

Wall-mounted washbasin.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

Vandal-resistant: shrouded basin, concealed trap.

Supplied with 1 electronic tap: flow rate pre-set at 3 lpm, infrared presence detection, adjustable duty flush, 230/12V mains supply.

Flat perforated waste, without screws: easy to clean and vandal-resistant.

Without overflow.

Supplied with trap.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 8.3kg.