**DELTA HD wall-hung urinal**

Polished satin 304 stainless steel - Rear inlet

Reference: **164770**

Specification description

Wall-hung individual rimless urinal.

Compatible with all standard frame systems on the market.

Bacteriostatic 304 stainless steel. Stainless steel thickness: 1.2mm.

Rear (recessed) inlet.

Vandal-resistant: recessed waste outlet, concealed trap and reinforced mounting frame.

Quick and easy to install from the front thanks to a stainless steel mounting frame.

Supplied with 1½" trap, fixing elements and theft prevention TORX security screws.

CE marked. Complies with European standard EN 13407 for 2L flush.

Weight: 7.5kg.