**TEMPOFIX 3 frame system for urinals**

Electronic urinal valve with mains supply

Reference: **543100**

Specification description

Frame system with electronic urinal valve:

Black powder-coated steel frame for wall-mounted installation.

Fixes to floor and load-bearing walls, anchoring bolts supplied.

Adjustable bracket 95 - 280mm.

Frame height can be can be adjusted 0 - 200mm.

Ø 50mm soil pipe with waterproof seal.

Delivered pre-mounted.

Compatible with solid wall finishes from 40 - 190mm.

Fitted with a TEMPOMATIC M½" electronic urinal valve:

Mains supply, 12V electronic control unit with solenoid valve, filter and stopcock.

Shock-resistant infrared presence detection sensor.

Detection distance, time flow and flow rate can be adjusted during installation.

Install a 230/12V transformer.

Detection delay is 3 seconds.

Automatic pre-rinse is possible.

Time flow pre-set at 3 seconds, can be adjusted from 3 - 12 seconds.

Hygienic duty flush every 24 hours after the last use: prevents vacuums.

Flow rate 0.3 L/sec. at 3 bar, can be adjusted.

Wall plate is flush to the wall.

Threaded rods can be cut to size.

Compatible with rain water.

Suitable for people with reduced mobility.

Technical features: see TEMPOMATIC urinal valve ref. 428200.

30-year warranty.