**TEMPOSOFT 2 time flow urinal valve**

Time flow 7 seconds

Straight, Soft-touch operation

Reference: **777807**

Specification description

Exposed time flow urinal valve.

For standard or siphon action urinals.

For wall-mounted, exposed installation.

Soft-touch operation.

Time flow ~7 seconds.

Flow rate pre-set at 0.15 L/sec. at 3 bar, can be adjusted.

Chrome-plated solid brass body M½".

Straight for inline inlets.

Compatible with rain water.

Suitable for people with reduced mobility.

30-year warranty.