

TEMPOSTOP urinal valve
Time flow 3 seconds
Recessed, with stainless steel wall plate

Reference: 777930


Specification description

Recessed time flow urinal valve. 

For standard or siphon action urinals.

For recessed installation.

Recessing depth can be adjusted from 20 to 35mm. 

Stainless steel wall plate Ø 130mm. 

Time flow ~3 seconds. 

Flow rate pre-set at 0.15 l/sec. at 3 bar, can be adjusted. 

Solid brass body M½".

30-year warranty.



This model does not have a waterproof recessing box. The installer must ensure that the recessing area is waterproof and any leaks or condensates can drain away (see installation guide).
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