**Deck-mounted twin hole mixer - 60 lpm**

Swivelling over spout L. 300mm H. 220mm

Can be installed close to the splashback

Reference: **5641T3UK**

Specification description

Deck-mounted twin hole mixer, M1/2" with 180mm centres.

Swivelling, tubular spout Ø 22mm H. 220mm L. 300mm with star-shaped flow straightener.

Water-free, guided valve heads with reinforced mechanisms.

Shock-resistant, ergonomic ball levers.

Flow rate 60 lpm at 3 bar achieved within first 90°.

Full flow 90 lpm at 3 bar.

Spout with smooth interior.

One-piece body and spout made from chrome-plated brass.

Reinforced fixings.

Can be installed close to the splashback.

30-year warranty.