**Be-Line drop-down support rail with leg, L. 850mm, anthracite**

Powder-coated metallised anthracite aluminium

Ø 42mm

Reference: **511963C**

Specification description

Be-Line drop-down support rail for people with reduced mobility.

In the lowered position use as a grab bar, as a support for standing and for assisting movement, for WCs or showers.

Allows side access in the raised position.

Removable: easy to remove with anti-theft locking system. Reduces the number of bars in a facility, allowing installation only when required.

Example: hotels or hospitals providing short-term accommodation for disabled people.

Drop-down rail retained in upright position. Slowed down descent.

Aluminium tube.

Rounded profile Ø 42mm with ergonomic flat front face that prevents rotation for an optimal grip.

Metallised anthracite powder-coated aluminium finish provides a good visual contrast with light-coloured walls.

Uniform surface for easy maintenance and hygiene.

Concealed fixings secured to wall by a 304 stainless steel plate, 5mm thick.

Supplied with stainless steel screws Ø 8 x 70mm for concrete walls.

Leg provides additional reinforcement when wall fixings are not enough.

Dimensions: 850 x 825 x 120mm.

Leg height can be adjusted from 760 - 780mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

Drop-down rail with 30-year warranty.

CE marked.