**TEMPOMATIC urinal valve**

Electronic, battery-operated

Cross wall 155mm

Reference: **428156**

Specification description

Cross wall electronic urinal valve:

CR123 6V lithium battery-operated, electronic control unit with solenoid valve, filter and stopcock M½".

Cross wall installation ≤ 155 mm.

Shock-resistant infrared presence detection sensor.

Detection distance, time flow and flow rate can be adjusted during installation.

Detection delay is 3 seconds.

Automatic pre-rinse is possible.

Time flow ~3 seconds, can be adjusted from 3 - 12 seconds.

Hygienic duty flush every 24 hours after last use: prevents vacuums.

Flow rate 0.3 L/sec. at 3 bar, can be adjusted.

Wall plate flush to the wall.

Threaded rod can be cut to size.

Compatible with rain water.

Suitable for people with reduced mobility.

30-year warranty.