**PMR XS wall-mounted washbasin**

Polished satin 304 stainless steel

With Ø 35mm right tap hole

Reference: **123400**

Specification description

Wall-mounted washbasin.

Basin internal diameter: 310mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

With Ø 35mm right tap hole.

Supplied with 1¼" waste.

Without overflow.

Supplied with fixings.

CE marked. Complies with European standard EN 14688.

Weight: 3.9kg.

30-year warranty.