**CANAL wall-mounted wash trough**

Polished satin 304 stainless steel - L. 1200mm

Without tap hole - left outlet

Reference: **122250**

Specification description

Wash trough for wall-mounting, 2 services - 1200mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 0.8mm for the bowl, 1.5mm for surround and fixing brackets.

Easy to install: no joint concealers to install, lightweight trough.

Water controls can be installed wall-mounted or deck-mounted.

Drainage on the left.

Without tap hole.

Supplied with M1"1/4 waste. Without overflow.

Supplied with fixings.

CE marked. Complies with European standard EN 14296.

Weight: 7.6kg.

30-year warranty.

Possible to add a bacteriostatic 304 stainless steel splashback (ref. 100250).

[Formerly ref: 0211250041]