**OUTDOOR time flow shower column**

Time flow, 2 showers

Anodised aluminium, ready to fit

Reference: **717520**

Specification description

Time flow shower column for outdoors:

Anodised aluminium shower column ready to fit.

Fitted with two showers.

Bottom inlet via stopcock F¾".

TEMPOSOFT 2 time flow valves for mixed water supply.

Soft-touch operation.

Time flow ~15 seconds.

Chrome-plated, tamperproof, scale-resistant ROUND shower heads with automatic flow rate regulation at 6 lpm at 3 bar.

Filters.

Access panel with isolation valve and purge.

Can easily be protected or taken apart in winter.

Suitable for people with reduced mobility.

30-year warranty.