**Mechanical basin mixer**

Single hole mechanical mixer H. 85mm, L. 135mm

Pop-up waste 11/4"

Reference: **2520**

Specification description

Deck-mounted mechanical basin mixer.

Single hole mechanical mixer H. 85mm L. 135mm with BIOSAFE hygienic outlet.

Ø 40mm classic ceramic cartridge with pre-set maximum temperature limiter.

Flow rate limited to 5 lpm at 3 bar.

Sculptured control lever.

Ergonomic pop-up waste 1 1/4" made from stainless steel.

PEX flexibles F3/8".

Reinforced fixing via 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Suitable for people with reduced mobility.

Mixer with 30-year warranty.