**SPORTING 2 time flow shower panel**

Time flow

Top or back inlet, anodised aluminium

Reference: **714700**

Specification description

Time flow shower panel:

Anodised aluminium and chrome-plated satin finish panel.

Adjustable connector for top or back inlets.

Slimline structure with concealed fixings.

Soft-touch operation.

Automatic mechanical flush with every use.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar, rain-effect spray.

Tamperproof fixed shower head with automatic flow rate regulation.

Adjustable spray.

Accessible filters and non-return valves.

Integrated stopcock.

M½" connection for mixed water supply.

Suitable for people with reduced mobility.

30-year warranty.