**SECURITHERM EP BIOSAFE pressure balancing basin mixer**

Single hole mechanical mixer with no spout, H. 95mm L. 110mm

Without pop-up waste, PEX flexibles

Reference: **2621EP**

Specification description

Deck-mounted mechanical basin mixer with pressure-balancing.

Single hole mechanical mixer H. 95mm L. 110mm.

No spout: BIOSAFE hygienic outlet integrated into the body.

Ø 35mm ceramic cartridge with pressure-balancing and pre-set maximum temperature limiter.

Anti-scalding safety: HW flow rate is reduced if CW supply fails (and vice versa).

Stable temperature regardless of pressure and flow rate variations in the system.

Securitouch thermal insulation prevents burns.

Thermal shocks are possible without removing the control lever or shutting off the cold water supply.

Mixer body with smooth interior and very low water volume (reduces bacterial development).

Flow rate limited to 4 lpm at 3 bar.

Solid control lever.

With no pop-up waste.

PEX flexibles F3/8" with rotating unions, filters and non-return valves.

Fixing reinforced by two stainless steel rods.

Mechanical mixer with SECURITHERM pressure-balancing ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.

Also available with copper tails.