**SECURITHERM BIOCLIP thermostatic sink mixer**

Wall-mounted sequential thermostatic mixer

Standard unions, removable stainless steel spout

Reference: **H9611S**

Specification description

Wall-mounted SECURITHERM thermostatic sink mixer.

Sequential thermostatic mixer: opens and closes with cold water.

No risk of cross flow between hot and cold water.

No non-return valves on the inlets.

Wall-mounted mixer supplied with 2 removable stainless steel spouts L.136mm.

Anti-scalding failsafe: shuts off automatically if cold or hot water supply fails.

Securitouch thermal insulation prevents burns.

Scale-resistant sequential thermostatic cartridge for sequential control of flow and temperature.

Temperature can be adjusted from cold water up to 40°C with maximum temperature limiter set at 40°C.

Thermal or chemical shocks are possible.

Body and spout with smooth interiors and low water volume.

Flow rate regulated at 7 lpm.

Chrome-plated brass body.

No manual contact thanks to Hygiene control lever L. 146mm.

Mixer with 150mm centres supplied with offset standard connectors M1/2" M3/4".

Mixer ideal for healthcare facilities, retirement homes, hospitals and clinics.

Sequential mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.