**BLACK BINOPTIC MIX electronic mixer**

Mains supply, H. 170mm

Long lever, smooth interior spout

Reference: **388MCHB**

Specification description

Deck-mounted matte black electronic basin mixer:

Independant IP65 electronic unit.

230/12V mains supply with transformer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set at 60 seconds every 24 hours after the last use).

Optimised active infrared presence detection at the end of the spout.

Body in chrome-plated brass.

Matte black chrome finish.

Fixings reinforced by 2 stainless steel rods.

PEX flexibles with filters and M3/8" solenoid valves.

Anti-blocking security.

Spout with smooth interior and low water volume (reduces niches where bacteria can develop).

Side temperature control lever with long lever and adjustable maximum temperature limiter.

Drop height: 170mm, for semi-recessed basins.

Suitable for people with reduced mobility.

30-year warranty.