**BLACK BINOPTIC MIX electronic mixer**

Mains supply, H. 250mm

Long lever, smooth interior spout

Reference: **398MCHB**

Specification description

Deck-mounted matte black electronic basin mixer:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush 60 seconds every 24 hours after last use).

Active, infrared presence detection, sensor at the end of the spout optimises detection.

Chrome-plated brass body.

Matte black chrome finish

PEX flexibles with filters and solenoid valves M⅜".

Fixing reinforced by 2 stainless steel rods.

Anti-blocking security.

Spout with smooth interior and low water volume (reduces bacterial development).

Side temperature control with adjustable maximum temperature limiter and long lever.

Drop height 250mm for countertop washbasins.

Suitable for people with reduced mobility.

30-year warranty.