**BLACK BINOPTIC MIX electronic mixer**

Battery-operated, H. 170mm

Long lever, smooth interior spout

Reference: **488MCHB**

Specification description

Deck-mounted matte black electronic basin mixer:

Independent IP65 electronic control unit.

123 6V Lithium batteries.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush 60 seconds every 24 hours after last use).

Active, infrared presence detection, sensor at the end of the spout optimises detection.

Chrome-plated brass body.

Matte black chrome finish.

PEX flexibles with filters and solenoid valves M⅜".

Fixing reinforced by 2 stainless steel rods.

Anti-blocking security.

Spout with smooth interior and low water volume (reduces bacterial development).

Side temperature control with adjustable maximum temperature and long lever.

Drop height 170mm for semi-recessed washbasins.

Suitable for people with reduced mobility.

30-year warranty.