**BLACK BINOPTIC electronic tap**

Battery-operated, H. 90mm

Smooth interior spout

Reference: **478035**

Specification description

Deck-mounted matte black electronic basin tap:

Independent IP65 electronic control unit.

123 6V Lithium battery-operated.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24hr after last use).

Active, infrared presence detection, sensor at the end of the spout optimises detection.

Chrome-plated brass body.

Matte black chrome finish.

PEX flexible with filter and solenoid valve M3/8".

Fixing reinforced by 2 stainless steel rods.

Anti-blocking safety.

Spout with smooth interior and low volume of water (reduces niches where bacteria can develop).

Suitable for people with reduced mobility.

30-year warranty.