**Backrest for Be-Line® shower seat**

Backrest for shower seats

Reference: **511929**

Specification description

Backrest for shower seat for disabled people and people with reduced mobility.

Large, designer model for shower seats ref. 511920C, 511920W, 511920BK, 511930C, 511930W and 511930BK.

Suitable for intensive use in commercial places or hospital environments.

Solid backrest made from high-resistant polymer.

Non-slip surface.

Matte white finish provides a good visual contrast with a dark wall.

Good resistance to chemical products and cleaning.

Anti-bacterial treatment: optimal protection against bacterial development.

4 concealed fixing points.

Supplied with Ø5 x 60mm screws and two Ø5 x 50mm screws.

Dimensions: 450 x 415 x 40mm.

Backrest for shower seat with a 30-year warranty.