**TEMPOSTOP time flow tap**

Anti-blocking version (AB)

Reference: **748110**

Specification description

Time flow basin tap for cross wall installation:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Chrome-plated solid brass body M½".

Control ≤ 200mm.

Anti-rotating pin and back-nut.

AB anti-blocking system: water will flow only when the push-button is released.

30-year warranty.

[Formerly ref: 741743]