**TEMPOSTOP time flow shower kit**

Time flow

Cross wall 200mm, ROUND shower head

Reference: **749110**

Specification description

Time flow shower kit for cross wall installation:

TEMPOSTOP time flow shower valve M½" for mixed water supply.

For walls ≤ 200mm.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated ROUND shower head, tamperproof and scale-resistant with automatic flow rate regulation.

Chrome-plated metal control.

Concealed fixing and anti-rotation pin.

Threaded rods can be cut to size.

30-year warranty.

[Formerly ref: 749159]