**TEMPOFLUX 1 direct flush valve**

Time flow direct flush WC valve

Cross wall 200mm

Reference: **761110**

Specification description

Time flow direct flush valve for cross wall installation:

For walls ≤ 200mm.

Soft-touch operation.

Time flow ~7 seconds.

Vacuum breaker.

Stopcock and flow rate/volume adjuster are integrated.

Chrome plated metal body.

Inline inlet M¾".

Connection washer Ø 32/55mm.

Threaded rod can be cut to size.

Upstream supply pipes: minimum Ø 20mm required at all points (including connectors).

Base flow rate: 1 l/sec at 1 bar dynamic pressure.

Compatible with rain water.

Suitable for people with reduced mobility.

30-year warranty.

[Formerly ref: 761200]