**SPEEDJET 2 anthracite air pulse hand dryer, with HEPA filter**

Air pulse

Anti-bacterial anthracite

Reference: **510624C**

Specification description

Metallised anthracite SPEEDJET 2 two-way air pulse hand dryer.

High speed electric hand dryer: dries in 10 - 12 seconds.

Comfort: warm air.

Anti-bacterial ABS for maximum hygiene.

Removable drip tray prevents any water dripping down the wall or onto the floor: easy to clean and service.

HEPA filter: retains 99.99% of airborne bacteria.

Infrared automatic activation.

Intelligent technology: stops automatically when hands are removed.

Anti-blocking: stops automatically if used continuously for more than 30 seconds.

Dimensions: 180 x 320 x 540mm.

Weight: 6.83kg.

Energy saving: heating element stops automatically at temperatures over 25°C.

Low energy consumption: 1,050W in non-heating mode, 1,550W in heating mode.

230V~ / 50Hz.

Airflow: 61 l/second. Air speed: 540km/h.

Noise level: 66 dBA.

Class II, IP21.

CE marked.

3-year warranty.