**BINOPTIC deck-mounted electronic soap dispenser**

Liquid or foam soap dispenser

Mains, chromed 304 stainless steel, 1.2m tube

Reference: **512121P**

Specification description

Deck-mounted electronic soap dispenser.

Liquid or foam soap dispenser.

No manual contact: hands are automatically detected by infrared cell.

Spout made from chrome-plated 304 stainless steel.

No waste pump dispenser.

Separate electronic unit for installation under the basin.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s or specialist foam soap.

Spout length: 105mm.

Supplied with a flexible tube 1.20m long for remote tanks.

30-year warranty.

CE marked.